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Pyranometers and pyrgeometers
Pyranometers and pyrgeometers measure the broadband shortwave and longwave irradiance, respectively. At Lampedusa three types of pyranometers, and one type of pyrgeometer, are used. The meteorlogical station is equipped with a Kipp and Zonen CM 11 pyranometer. Eppley Precision Spectral Pyranometers (PSP) and a Black and White pyranometer are used during campaigns, and for calibration purpose. The PSP is a WMO class one radiometer; the sensor is a thermopile, covered by two polished optical Schott glass domes. This configuration produces a uniform spectral responsivity throughout the region 0.28-2.8 micron.
The CM 11 is a secondary standard pyranometer. The sensor is covered by two optical glass domes, and is sensitive to radiation between 0.3 and 2.8 micron.
The Black and White pyranometer has a differential thermopile, connected to the black and white segments of the sensor, which is enclosed in a Schott optical glass hemisphere, that uniformly transmits radiation between 0.28 and 2.8 micron.
The Eppley Precision Infrared Pyranometer (PIR) is used for the measurement of the broadband infrared radiation. The PIR is sensitive to radiation between 4 and 50 micron. It is constituted by a thermopile sensor, covered by a silicon dome, internally coated with an interference filter with a transmission range of approximately 3.5 to 50 micron.
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Eppley Precision Infrared Radiometer (PIR)
Pyranometre și pygeometre
Pyranometrele și pyrgeometrele măsoară intensitatea undelor de undă în bandă largă și, respectiv, iradierea lungimilor. La Lampedusa sunt utilizate trei tipuri de piranometre și un tip de pygeometru. Stația meteorologică este echipată cu un piranometru Kipp și Zonen CM 11. Spectral Spectral Pyranometers (PSP) și un piranometru alb-negru sunt folosite în timpul campaniilor și în scopul calibrării. PSP este un radiometru clasa WMO; senzorul este un termopil, acoperit de două cupole optice lustruite de sticlă Schott. Această configurație produce o reacție spectrală uniformă în întreaga regiune de 0,28-2,8 microni.
CM 11 este un piramometru secundar standard. Senzorul este acoperit de două cupole optice din sticlă și este sensibil la radiații între 0,3 și 2,8 microni.
Piranometrul negru și alb are o termopilă diferențială, conectată la segmentele alb-negru ale senzorului, care este închisă într-o emisferă de sticlă optică Schott, care transmite uniform radiația între 0,28 și 2,8 microni.
Pentru măsurarea radiației infraroșii în bandă largă se utilizează Pyranometrul cu infraroșu de precizie Eppley (PIR). PIR este sensibil la radiații între 4 și 50 microni. Acesta este constituit dintr-un senzor termopilat, acoperit de o cupolă de siliciu acoperită în interior cu un filtru de interferență cu un interval de transmisie de aproximativ 3,5 până la 50 de microni.
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Eppley Radiometru cu infrarosu de precizie (PIR)
[image: http://www.lampedusa.enea.it/strumenti/pyranometers_pyrgeometers/foto2.jpg]
Eprană Pyranometru Spectral de Precizie, cu ventilator.
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