SolarSIM-G
The next evolution of SolarSIM
With the SolarSIM-G, Spectrafy’s engineers have taken the SolarSIM technology to the next level and built a product that enables accurate and affordable measurement of the complete, global solar spectrum and total global irradiance.
For applications where measurement of the global solar spectrum is a must, the SolarSIM-G sets a new standard for accuracy, affordability and ease of use.
Much like it’s sister, the D2, the SolarSIM-G uses low-cost silicon photodiodes and bandpass interference filters to make precise measurements of the solar spectrum in several narrow wavelength bands. While the D2 is configured to measure the direct solar spectrum, Spectrafy’s engineers have optimised the SolarSIM-G’s hardware and software to measure and resolve the complete global solar spectrum and total globalirradiance.
Applications for the SolarSIM-G include solar resource assessment, PV panel development, certification and O&M, agricultural monitoring, UV index measurement, material testing and even multi- and hyper-spectral imaging.
The SolarSIM-G can be used in horizontal or tilted applications, thereby making it applicable to all flat-plate solar technologies and installations.
Purchase and lease options are available.
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The Data
The new standard in global irradiance data
The SolarSIM-G is a versatile device that can provide the function of a pyranometer and multiple spectroradiometers, all in one. As a result the SolarSIM-G can provide an unparalleled quantity and quality of data – over 4,000 data points per time stamp! Your SolarSIM-G can be configured to deliver any or all of the following:
Global Horizontal (or tilted) Irradiance (GHI/GTI)
The SolarSIM-G provides an accurate measurement of global irradiance (horizontal or tilted), under any sky conditions, over the complete 280-4000nm spectral range. The SolarSIM-G can also be configured to provide GHI/GTI over any custom  spectral range – great for quantifying useable fractions for PV, PAR values or UV doses.
Global Spectral Irradiance
The SolarSIM-G is capable of resolving the global solar spectral irradiance (horizontal or tilted), under any sky conditions, over the complete spectral range of 280 – 4000nm, with 1nm resolution. If you don’t need full-range, no problem. The SolarSIM-G can also be configured for just the 280-1200nm range.
The SolarSIM-G also provides accurate measurements of the ambient temperature, pressure and humidity.
SolarSIM-G
Următoarea evoluție a SolarSIM
Cu ajutorul tehnologiei SolarSIM-G, inginerii Spectrafy au preluat tehnologia SolarSIM la nivelul următor și au construit un produs care permite măsurarea exactă și la prețuri accesibile a spectrului solar global global și a iradierii totale globale.
Pentru aplicațiile în care măsurarea spectrului solar global este o necesitate, SolarSIM-G stabilește un nou standard pentru acuratețe, accesibilitate și ușurință în utilizare.
La fel ca și sora, D2, SolarSIM-G folosește fotodiodele de siliciu ieftine și filtrele de interferență de bandă pentru a face măsurători precise ale spectrului solar în câteva benzi înguste de lungime de undă. În timp ce D2 este configurat pentru a măsura spectrul solar direct , inginerii Spectrafy au optimizat hardware-ul și software-ul SolarSIM-G pentru a măsura și rezolva întregul spectru solar global și iradiența globală totală .
Aplicațiile pentru SolarSIM-G includ evaluarea resurselor solare, dezvoltarea panoului PV, certificarea și O & M, monitorizarea agriculturii, măsurarea indicelui UV, testarea materialelor și chiar imaginile multi- și hiperspectrale.
SolarSIM-G poate fi utilizat în aplicații orizontale sau înclinate, făcându-l astfel aplicabil tuturor tehnologiilor și instalațiilor solare plate.
Sunt disponibile opțiuni de cumpărare și de închiriere.
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Datele
Noul standard în datele de iradiere globală
SolarSIM-G este un dispozitiv versatil care poate oferi funcția unui piramometru și a mai multor spectroradiometre, toate într-unul. Ca urmare, SolarSIM-G poate oferi o cantitate și o calitate de neegalat de date - peste 4.000 de puncte de date pe ștampilă de timp! SolarSIM-G dvs. poate fi configurat pentru a furniza oricare dintre următoarele:
Iradierea orizontală (orizontală) (GHI / GTI)
SolarSIM-G oferă o măsurare exactă a iradierii globale (orizontală sau înclinată), în orice condiții de cer, pe întreaga gamă spectrală de 280-4000nm. SolarSIM-G poate fi de asemenea configurat pentru a furniza GHI / GTI pe orice spectru personalizat - excelent pentru cuantificarea fracțiunilor utilizabile pentru valori PV, PAR sau doze UV.
Iradierea spectrală globală
SolarSIM-G este capabil să rezolve irradiența spectrală globală (orizontală sau înclinată), în orice condiții de cer, pe întreg spectrul spectral de 280 - 4000nm, cu rezoluție de 1nm. Dacă nu aveți nevoie de gamă completă, nici o problemă. De asemenea, SolarSIM-G poate fi configurat doar pentru gama de 280-1200nm.
SolarSIM-G oferă, de asemenea, măsurători exacte ale temperaturii ambiante, presiunii și umidității.
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