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About Us
Graphene Batteries AS is a Norwegian SME engaged in development of Li-S battery technology enhanced with graphene derivatives. GB has developed a sulfur cathode based on proprietary method. Graphene derivatives are supplied by GB's sister company Abalonyx AS. With these results, the ambition is now to set up a pilot assembly line and commercialize Li-S batteries for the unmanned airplanes market within approximately 2 years with further scale-up to follow.
Despre noi

 Grafen Baterii AS este un IMM norvegian angajat în dezvoltarea tehnologiei bateriei Li-S îmbunătățită cu derivați de grafen. GB a dezvoltat o catod de sulf bazat pe metoda de proprietate. Derivații de grafen sunt furnizați de compania soră a GB, Abalonyx AS. Cu aceste rezultate, ambiția este acum de a înființa o linie de asamblare pilot și comercializarea bateriilor Li-S pentru piața avioanelor fără pilot în termen de aproximativ 2 ani, cu scară suplimentară de urmat.
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Li-S Battery Technology
A high surface area porous carbon with inter connected network is utilised as support for both anode and cathode. This structure was developed by Graphene Batteries and has already shown extremely promising results when applied as both anode and cathode support. At the cathode it provides a strong and flexible host structure which can accommodate the volume expansion experienced by sulfur during cycling. At the anode it provides stabilisation of the lithium-electrolyte interface, which will allow reduction of the electrolyte/sulfur ratio from a typical "excess" value of 10 µL/mg to a more commercially relevant value of 3 µL/mg. 
Tehnologia bateriilor

 Li-S O suprafață mare de carbon poros cu rețea interconectată este utilizată ca suport atât pentru anod, cât și pentru catod. Această structură a fost dezvoltată de Grafene Batteries și a arătat deja rezultate extrem de promițătoare atunci când este aplicată atât ca suport anodic, cât și catod. La catod oferă o structură gazdă puternică și flexibilă, care poate găzdui expansiunea volumului experimentat de sulf în timpul ciclismului. La anod se asigură stabilizarea interfeței litiu-electrolit, ceea ce va permite reducerea raportului electrolit/sulf de la o valoare tipică "în exces" de 10 μL/mg la o valoare mai relevantă din punct de vedere comercial de 3 μL/mg.  
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